Sheet1

Spectrometer (both arms) Proposed Version April 14, 1997

Components/module Mod # Module FlexR FlexL DSL DSS MSDR MSDL MSS3R MSS3L MSS4R MSS4L T1 T2 T3 T4 T5 8 Mod1 2 2 24 24 2 2 2 Frame 1+2 4 Mod2 1 1 32 1 1 4 Frame 3 4 Mod7-T2 1 1 24 1 1 3 Frame 4 6 Mod4-T4 1 16 1 4 Frame 5+6 12 Mod4-T5 1 16 1 4 Frame 7+8 6 Mod5-T4 1 12 1 3 Frame 6 28 Mod5-T5 1 16 1 3 Frame 7+8 8 Mod6 1 1 32 1 1 4 Frame 5+6 8 Mod7-T3 1 1 24 1 1 3 Frame 7+8

Total components Module FlexR FlexL DSL DSS MSDR MSDL MSS3R MSS3L MSS4R MSS4L T1 T2 T3 T4 T5 Mod1 16 16 192 192 16 16 0 0 0 0 16 0 0 0 0 Mod2 4 4 0 128 0 0 0 0 4 4 0 16 0 0 0 Mod7-T2 4 4 0 96 0 0 4 4 0 0 0 12 0 0 0 Mod4-T4 0 6 0 96 0 0 0 0 0 6 0 0 0 24 0 Mod4-T5 0 12 0 192 0 0 0 0 0 12 0 0 0 0 48 Mod5-T4 0 6 0 72 0 0 0 6 0 0 0 0 0 18 0 Mod5-T5 0 28 0 448 0 0 0 0 0 28 0 0 0 0 84 Mod6 8 8 0 256 0 0 0 0 8 8 0 0 32 0 0 Mod7-T3 8 8 0 192 0 0 8 8 0 0 0 0 24 0 0 Total 40 92 192 1672 16 16 12 18 12 58 16 28 56 42 132

Flexcable: 132 DS: 1864 MS: 132 Sensors: 274 ch/DS 64 channel: 119296

Remark1 : Frame 4: single-sensor module (mod3) + 2 Mod2 replaced by 4 new modules of type Mod7 with T2 sensors -> 2 Types of M substrates less (MSS1R and MSS1L), 6 instead of 5 sensors Remark2 : Frame 5: remove Mod8 by using Mod 6 -> 1 module type less, no mixing of sensor types on modules, no partially assembled MS, higher granularity, slightly more channels

Page 1