BRAHMS

Beam-Beam Counter

Trigger System

~ 99% efficiency ~ 1cm vertex resolution

Level 0

Level 1

Level 2

Centrality Detector (Silicon Strips)

|η| < 2.5 10% Centrality Cut

SPEC Trigger (Forward Spectrometer)

Hodo’s + DC’s

(Expected charged multiplicity for 15-30 GeV/c setting < 0.8[@2.1^o])

Track Finding Trigger (+ PID)

Hodo + DC’s (or Trigger Chambers) + Logic Similar as E859+E866

Similar as E866 Forward Spec. Trigger

p, correlations, resonances

MID

FS

BB BB

Multiplicity

x x x x x

Hodo’ sDC’ s